|  |  |
| --- | --- |
| **Quotation Called on** |  |
| **Quotation Closed on** |  |
| **No. of Quotations received** |  |
| **Quotation Opened on** |  |

**TEC SCHEDULE**

**Schedule for Technical Evaluation Committee**

**Faculty of Veterinary Medicine & Animal Science**

**Item: Purchasing of …………………………………………….**

**Department: ……………………………………………………….Faculty of Veterinary Medicine & Animal Science**

**Quotations were received from following suppliers**

1. **ITED Technologies & Solutions (Pvt)Ltd 2. Inventek Consolidated 3. DataLOG Information Systems (Pvt)Ltd 4 Pixalogy (Pvt) Ltd**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Our requirement** | **No of Items****purchased** | **Supplier No 01** | **Supplier No 02** | **Supplier No 03** | **Supplier No 04** |
| Is bid completed Signed, StampedAny alteration \*\* |  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| VAT - Registered |  |  |  |  |  |
| VAT- Not RegisteredIf not letter from Inland Revenue Dept. |  |  |  |  |  |
|  |  |  |  |  |
| **Specification of the purchasing item** |  |  |  |  |  |
| Digital Video Recorder | 01 |  |  |  |  |
| Video Compression: H.265 Pro+/H.265 Pro/H.265 or equivalent |  | Yes | Yes | Yes | Yes |
| Video input: HDTVI/AHD/CVI/CVBS/IP |  | Yes | Yes | Yes | Yes |
| Camera input: 32 or better |  | Yes | Yes | Yes | Yes |
| Signal transmission: 800m for 1080p and 1200m for 720p HDTV I or better |  | Yes | Yes | Yes | Yes |
| Hard Drives: 2 SATA interfacesShall fully support the below mentioned cameras. |  | Yes | Yes | Yes | Yes/Up to 10TB  |
| Video Bit Rate: 32 Kbps-6 Mbps or better |  | Yes | Yes | Yes | Yes |
| Stream Type: Video/ Video & Audio |  | Yes | Yes | Yes | Yes |
| Synchronous Playback: 16-channel or better |  | Yes | Yes | Yes | Yes/ 16 Channel |
| 5 MP Bullet Camera | 10 |  |  |  |  |
| Analog HD output |  | Yes | Yes | Yes | Yes |
| IR distance: 20m or better |  | Yes | Yes/40 m | Yes | Yes/20 m |
| Shall be suitable for outdoor mounting |  | Yes | Yes | Yes | Yes |
| With a suitable lenses for the location of installation to provide maximum visibility (lens sizes from 2.8mm -12 mm may be used) |  | Yes | Yes | Yes | Yes / as per Location |
| Video Frame Rate: 2560 x 1944 @ 20fps or better |  | Yes | Yes | Yes | Yes |
| Adjustment Range: Pan: 0° to 360°; Tilt:0° to 180°; Rotate: 0° to 360° |  | Yes | Yes | Yes |  Yes / 40 m |
| 5 MP Bullet Camera | 09 | Yes | Yes |  |  |
| Analog HD output |  | Yes | Yes | Yes | Yes |
| IR distance: 80m or better |  | Yes | Yes |  40m | Yes |
| Shall be suitable for outdoor mounting |  | Yes | Yes | Yes | Yes |
| Video Frame Rate: 2560 x 1944 @ 20fps or better |  | Yes | Yes | Yes | Yes |
| Adjustment Range: Pan: 0° to 360°; Tilt:0° to 180°; Rotate: 0° to 360° |  | Yes | Yes | Yes | Yes |
| 4TB or better SATA Hard Disk Drive | 02 |  |  | Yes | Yes |
| Display 2: 32 inch or better LED Television and a suitable TV wall mount | 01 | Yes | Yes | Yes | Yes |
| Display 1: 24 inch or better LED Television and a suitable TV wall mount | 01 | Yes | Yes | Yes | Yes |
| HDMI extender and HDMI cable (about 25m) to connect the second display) | 01 | Yes | Yes | Yes | Yes |
| Network Cabinet | 01 | Yes | Yes | Yes | Yes |
| Installation charges (shall include labor charges, and all other charges for relevant accessories such as power adapters, jacks, cables, casings, conduits, video balloons, and underground cable laying when necessary between the buildings).All the cables laid between the buildings (outside) shall be carried out in PVC pipes and shall be laid according to an acceptable standard by the university. Two cameras have to be amounted to GI pipes (1 "4") |  | Yes | Yes | Yes | Yes |
| Warranty: 2 year comprehensive |  | Not Mentioned | Yes |  No/1 Year | Yes |
| Unit price |  | 841,400.00 | 1,361,620.00 | 679,280.00 | Not Mentioned |
| VAT |  | 126,210.00 | - | - |
| **TOTAL** |  | **967,610.00** | **1,361,620.00** | **679,280.00** |

\*\* Insert “Y” in answer is Yes and “N” if answer is No.
Prepared by:

Chairman/TEC:………………………………… Member- TEC:……………………………………………….. Member- TEC:……………………………